(footprint "CP_Elec_8x10.5"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SMD capacitor, aluminum electrolytic, Vishay 0810, 8.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
	(tags "capacitor electrolytic")
	(property "Reference" "REF**"
		(at 0 -5.3 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CP_Elec_8x10.5"
		(at 0 5.3 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -5.6 -2.51)
		(end -4.6 -2.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.1 -3.01)
		(end -5.1 -2.01)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.36 -3.295563)
		(end -4.36 -1.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.36 -3.295563)
		(end -3.295563 -4.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.36 3.295563)
		(end -4.36 1.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.36 3.295563)
		(end -3.295563 4.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -3.295563 -4.36)
		(end 4.36 -4.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -3.295563 4.36)
		(end 4.36 4.36)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 4.36 -4.36)
		(end 4.36 -1.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 4.36 4.36)
		(end 4.36 1.51)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -6.15 -1.5)
		(end -6.15 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -6.15 1.5)
		(end -4.5 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.5 -3.35)
		(end -4.5 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.5 -3.35)
		(end -3.35 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.5 -1.5)
		(end -6.15 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.5 1.5)
		(end -4.5 3.35)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.5 3.35)
		(end -3.35 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -3.35 -4.5)
		(end 4.5 -4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -3.35 4.5)
		(end 4.5 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 4.5 -4.5)
		(end 4.5 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 4.5 -1.5)
		(end 6.15 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 4.5 1.5)
		(end 4.5 4.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 6.15 -1.5)
		(end 6.15 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 6.15 1.5)
		(end 4.5 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.25 -3.25)
		(end -4.25 3.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.25 -3.25)
		(end -3.25 -4.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.25 3.25)
		(end -3.25 4.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -3.562278 -1.5)
		(end -2.762278 -1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -3.25 -4.25)
		(end 4.25 -4.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -3.25 4.25)
		(end 4.25 4.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -3.162278 -1.9)
		(end -3.162278 -1.1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 4.25 -4.25)
		(end 4.25 4.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_circle
		(center 0 0)
		(end 4 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3.7 0)
		(size 4.4 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(pad "2" smd roundrect
		(at 3.7 0)
		(size 4.4 2.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_8x10.5.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
