(footprint "R_2220"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 2220 (5750 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -3.65 0)
		(layer "F.SilkS")
		(uuid "282e810f-0c45-4ce2-a07d-76ac615ec55f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_2220"
		(at 0 3.65 0)
		(layer "F.Fab")
		(uuid "ff1564c2-6901-4455-99f9-6f7b467a88be")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2b06edb7-ec9d-4deb-a958-e621d14e5600")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0c7177e0-7dbf-4764-874d-d8d1076b64b8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.5 -2.7)
		(end 1.5 -2.7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2dfc51d6-21f7-4dc6-b30c-9ec11fd6565c")
	)
	(fp_line
		(start -1.5 2.7)
		(end 1.5 2.7)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "45fde2f9-0323-4ab0-bdda-8260a919998e")
	)
	(fp_rect
		(start -4.208 -2.95)
		(end 4.335 2.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "09047330-86c0-44f3-bb18-38cab130a923")
	)
	(fp_rect
		(start -2.85 -2.5)
		(end 2.85 2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "893bb6d7-afba-4b29-9a9d-2e7e500f9680")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "73cbffe1-ec0e-4167-9790-30b9b3b11666")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -3 0)
		(size 2 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.075)
		(uuid "d34eec52-63bd-4f2d-9a81-800398036218")
	)
	(pad "2" smd roundrect
		(at 3 0)
		(size 2 5.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.075)
		(uuid "8a4fa07e-8e16-4585-a8b2-9a8aa7b7dcaa")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5750Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
