(footprint "CP_Elec_18x22"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SMD capacitor, aluminum electrolytic, Vishay 1821, 18.0x22.0mm, http://www.vishay.com/docs/28395/150crz.pdf")
	(tags "capacitor electrolytic")
	(property "Reference" "REF**"
		(at 0 -10.55 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CP_Elec_18x22"
		(at 0 10.55 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -12.1 -7.31)
		(end -9.85 -7.31)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -10.975 -8.435)
		(end -10.975 -6.185)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -9.61 -8.545563)
		(end -9.61 -5.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -9.61 -8.545563)
		(end -8.545563 -9.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -9.61 8.545563)
		(end -9.61 5.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -9.61 8.545563)
		(end -8.545563 9.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -8.545563 -9.61)
		(end 9.61 -9.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -8.545563 9.61)
		(end 9.61 9.61)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 9.61 -9.61)
		(end 9.61 -5.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 9.61 9.61)
		(end 9.61 5.06)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -11.4 -5.05)
		(end -11.4 5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -11.4 5.05)
		(end -9.75 5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.75 -8.6)
		(end -9.75 -5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.75 -8.6)
		(end -8.6 -9.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.75 -5.05)
		(end -11.4 -5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.75 5.05)
		(end -9.75 8.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.75 8.6)
		(end -8.6 9.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -8.6 -9.75)
		(end 9.75 -9.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -8.6 9.75)
		(end 9.75 9.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 9.75 -9.75)
		(end 9.75 -5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 9.75 -5.05)
		(end 11.4 -5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 9.75 5.05)
		(end 9.75 9.75)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 11.4 -5.05)
		(end 11.4 5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 11.4 5.05)
		(end 9.75 5.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -9.5 -8.5)
		(end -9.5 8.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -9.5 -8.5)
		(end -8.5 -9.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -9.5 8.5)
		(end -8.5 9.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -8.5 -9.5)
		(end 9.5 -9.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -8.5 9.5)
		(end 9.5 9.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -8.499342 -2.5)
		(end -6.699342 -2.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -7.599342 -3.4)
		(end -7.599342 -1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 9.5 -9.5)
		(end 9.5 9.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_circle
		(center 0 0)
		(end 9 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -6.75 0)
		(size 8.8 9.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.028409)
	)
	(pad "2" smd roundrect
		(at 6.75 0)
		(size 8.8 9.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.028409)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_18x22.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
