(footprint "CP_TANT_A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
	(tags "capacitor tantalum")
	(property "Reference" "REF**"
		(at 0 -1.75 0)
		(layer "F.SilkS")
		(uuid "762a0f39-e27f-4642-81f8-9a4fa4542ded")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CP_TANT_A"
		(at 0 1.75 0)
		(layer "F.Fab")
		(uuid "1e97364d-c8ee-4b6e-ab2d-624580c18770")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "730275c3-4bca-47f2-ad1a-8dd40fdc1af5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a21f9aa1-96a7-4424-9904-36bde435adb5")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_poly
		(pts
			(xy -0.3048 -0.889) (xy -0.3048 0.889) (xy 0.4572 0.889) (xy 0.2462 0.889) (xy -0.0078 0.635) (xy -0.0078 -0.635)
			(xy 0.2462 -0.889) (xy 0.4572 -0.889)
		)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "ed36e139-28d8-45b2-86cf-4c727d188edf")
	)
	(fp_rect
		(start -2.31 -1.05)
		(end 2.31 1.05)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "e6df087f-101c-4785-809b-faa8030d353a")
	)
	(fp_line
		(start -1.6 -0.4)
		(end -1.6 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6d658a77-62d5-49e8-990e-9ee18d5cd33f")
	)
	(fp_line
		(start -1.6 0.8)
		(end 1.6 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "017a9bff-23b6-4da1-9eea-5f02883e7e5a")
	)
	(fp_line
		(start -1.2 -0.8)
		(end -1.6 -0.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "842e6dac-0a7a-4f24-a640-ede587ec083b")
	)
	(fp_line
		(start 1.6 -0.8)
		(end -1.2 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "be9bf1d7-8058-4556-b568-5c97834dce0e")
	)
	(fp_line
		(start 1.6 0.8)
		(end 1.6 -0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "19b3e158-860a-4b18-a2c9-2ec717d993e4")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "3beeea8a-44bf-4e47-aa82-eff1eb7445f4")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.3525 0)
		(size 1.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.179856)
		(uuid "0c2eda61-c24e-4752-846c-8046b16fc5c7")
	)
	(pad "2" smd roundrect
		(at 1.3525 0)
		(size 1.6 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.179856)
		(uuid "4e301132-6434-436d-8d4d-042157b1aca9")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
