(footprint "CP_TANT_B"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC-7352 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
	(tags "capacitor tantalum")
	(property "Reference" "REF**"
		(at 0 -2.35 0)
		(layer "F.SilkS")
		(uuid "98bcb361-8b43-44a3-bd9e-bebe36474ec1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CP_TANT_B"
		(at 0 2.35 0)
		(layer "F.Fab")
		(uuid "337d15fe-15df-4dd9-8454-c6626081acd0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "09bee554-b44c-442a-9b28-dd52d559dc32")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d9bf1476-dc5c-4032-9134-e090872249db")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_arc
		(start -1.041405 -1.4732)
		(mid -0.664234 -1.316971)
		(end -0.508005 -0.9398)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "7d55325f-0b5a-4294-a4ac-15ba10679a8e")
	)
	(fp_arc
		(start -0.508005 0.9398)
		(mid -0.664234 1.316971)
		(end -1.041405 1.4732)
		(stroke
			(width 0.2)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "d1ea61dc-e663-42e9-8f6e-b391684e1799")
	)
	(fp_poly
		(pts
			(xy 1.422395 -1.4732) (xy 0.240578 -1.4732) (xy 0.240447 1.4732) (xy 1.4224 1.4732) (xy -1.673235 1.4732)
			(xy -0.508004 1.4732) (xy -0.507997 -1.4732) (xy -1.673235 -1.4732)
		)
		(stroke
			(width 0.2)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "95048ca4-0cfa-4dec-9a7f-485790f7452a")
	)
	(fp_rect
		(start -2.5362 -1.65)
		(end 2.5616 1.65)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "4537c100-11d2-4f68-8567-f0c33870be4d")
	)
	(fp_line
		(start -1.75 -0.7)
		(end -1.75 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "eb945573-d19a-48b7-9001-084ee01e87f7")
	)
	(fp_line
		(start -1.75 1.4)
		(end 1.75 1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "088c0937-4115-43ae-9ba9-5e2cccf69df8")
	)
	(fp_line
		(start -1.05 -1.4)
		(end -1.75 -0.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d1b78207-db84-4f2a-837b-1ac0e1e56955")
	)
	(fp_line
		(start 1.75 -1.4)
		(end -1.05 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9071129d-2602-407c-b94c-586d32ed276b")
	)
	(fp_line
		(start 1.75 1.4)
		(end 1.75 -1.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4456d400-d1d0-4d6d-a7b9-e986ca7cd448")
	)
	(fp_text user "${REFERENCE}"
		(at -0.0508 0 0)
		(layer "F.Fab")
		(uuid "4a432d1d-0624-49fd-b52e-d3b5d06b59af")
		(effects
			(font
				(size 0.88 0.88)
				(thickness 0.13)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.54 0)
		(size 1.45 2.39)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.186567)
		(uuid "dd69c266-f22e-401b-aa88-f66a59f4fca1")
	)
	(pad "2" smd roundrect
		(at 1.54 0)
		(size 1.45 2.39)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.186567)
		(uuid "ec779845-f0eb-4ec1-a775-1a0e7e6cac87")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
