(footprint "R_1210"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -2.3 0)
		(layer "F.SilkS")
		(uuid "83d49f2c-54c2-4412-8d07-85f7296fe0ab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_1210"
		(at 0 2.3 0)
		(layer "F.Fab")
		(uuid "98d50a2f-52d0-4c80-a110-ea8a1f0ed8f0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "14c1f2ef-ef2e-4bfe-a85c-ceac264a2065")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "44826f92-4096-4af9-9381-804d046c2253")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.77788 -1.27)
		(end 0.74612 -1.27)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c8f4f2be-f676-4b7e-80b5-c5e254952f4c")
	)
	(fp_line
		(start -0.77788 1.27)
		(end 0.74612 1.27)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "27db740a-d41e-4b64-8f5d-64d11afb77c4")
	)
	(fp_rect
		(start -2.427 -1.6)
		(end 2.427 1.6)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "5fdd80d1-a983-4bd1-a74c-4a2e7a3701ce")
	)
	(fp_rect
		(start -1.6 -1.25)
		(end 1.6 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "2eedb5e3-fc20-438f-bbbe-294de0725a1d")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "a8a66bb0-5599-48d1-8252-4d5d4e32b8c3")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.68276 0)
		(size 1.25 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "31a9fba5-6c09-4402-895a-89ed3d1f3171")
	)
	(pad "2" smd roundrect
		(at 1.651 0)
		(size 1.25 2.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "0cfa4e32-e378-4392-b185-2f7ad6f5f00e")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
