(footprint "C_1812"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1812 (4532 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
		(uuid "88fbfc6f-9ffc-4da4-9874-6a103015c90d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_1812"
		(at 0 2.65 0)
		(layer "F.Fab")
		(uuid "ab835028-5a19-494e-9d0e-7f4868831df9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e10fadcf-992e-49d6-9502-b389b22ed6e4")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2fb8b81c-a789-4b66-8050-f25afa5d5caa")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.287 -1.5998)
		(end 1.313 -1.5998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "840e5c89-f930-4c5b-9a08-36f04f543629")
	)
	(fp_line
		(start -1.187 1.6002)
		(end 1.213 1.6002)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0663c014-9fd9-4da1-9ce7-d73def34c82c")
	)
	(fp_line
		(start 0.013 1.6002)
		(end 0.013 -1.5998)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6a0f59bb-f7e7-4f7a-bde2-a44f675b75cb")
	)
	(fp_rect
		(start -3.381 -1.95)
		(end 3.381 1.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "72c2beca-95f3-473b-a62e-e8f8e32ab55d")
	)
	(fp_rect
		(start -2.25 -1.6)
		(end 2.25 1.6)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "30669c74-32c4-4373-a544-55fdac36f217")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "aa6a23b5-04db-468a-ba3c-8b3e14a7b094")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.35 0)
		(size 1.6 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.178571)
		(uuid "27673394-b3f7-425a-8274-89303d522d87")
	)
	(pad "2" smd roundrect
		(at 2.35 0)
		(size 1.6 3.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.178571)
		(uuid "54dfda2f-b2aa-4ac8-ae92-3ef9db0e0569")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1812_4532Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
