(footprint "C_1206"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -1.85 0)
		(layer "F.SilkS")
		(uuid "186062fb-65e1-4e1b-a61f-5e652a65e60d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_1206"
		(at 0 1.85 0)
		(layer "F.Fab")
		(uuid "a82a1324-ea57-45fe-910d-07a4e02fe184")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e36e3a8c-0eec-4d03-99de-f8d0d8d86c04")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "c0d84bcb-b088-4475-a389-df477b5b5e2a")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.8 -0.9)
		(end 0.8 -0.9)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "45d65cd2-2282-4e83-b65c-75319fa9bbcf")
	)
	(fp_line
		(start -0.8 0.9)
		(end 0.8 0.9)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "5b0f8b8c-ce20-4ed4-ba5c-61b97b473219")
	)
	(fp_line
		(start 0 0.9)
		(end 0 -0.9)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ed10e19-a1cd-4431-8d7b-32259dced070")
	)
	(fp_rect
		(start -2.3 -1.15)
		(end 2.3 1.15)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "54867e9a-c8a2-4d48-bba0-7975a996b129")
	)
	(fp_rect
		(start -1.6 -0.8)
		(end 1.6 0.8)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "278cfce4-efc8-4ac3-90a6-0f62ea7680be")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "efe3adb6-8cb4-4f64-99de-c8e7c59042da")
		(effects
			(font
				(size 0.8 0.8)
				(thickness 0.12)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.524 0)
		(size 1.15 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "f14e12a8-66e6-4390-9045-c388222b577c")
	)
	(pad "2" smd roundrect
		(at 1.524 0)
		(size 1.15 1.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.217391)
		(uuid "c79d92ca-68bc-48b1-9dd6-6a57baefe8c4")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
