(footprint "C_0805"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -1.68 0)
		(layer "F.SilkS")
		(uuid "49ba145d-1518-4115-9136-ec82df477016")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_0805"
		(at 0 1.68 0)
		(layer "F.Fab")
		(uuid "3defff50-88bb-4012-a42d-1254c988e9e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "96de039f-67f5-4e8f-a4d1-9e6eabf64566")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "10df5b95-ccc9-44a2-96b7-02ecbc56f0bb")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.261252 -0.635)
		(end 0.261252 -0.635)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "74b8b5ab-f6f8-4010-9fb0-1388e5bcb2f1")
	)
	(fp_line
		(start -0.261252 0.635)
		(end 0.261252 0.635)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0ce60668-65e3-4e25-b3ee-28f9453a0f73")
	)
	(fp_line
		(start 0 0.635)
		(end 0 -0.635)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6a1f3778-723a-42f9-beac-59d8b3609df2")
	)
	(fp_rect
		(start -1.7 -0.98)
		(end 1.7 0.98)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "1ba17410-7d3a-4ac0-b3fb-0fc8cb9d48e7")
	)
	(fp_rect
		(start -1 -0.625)
		(end 1 0.625)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "1d501cf5-3aa2-4c0d-ab93-c86181c15be0")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "c14ab70c-b5f6-4a57-b356-c49d02239b75")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "4d74c07b-3da0-4212-897a-28aebc680519")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "7db9fb8e-7120-43eb-8322-0c609a96d9e0")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
