(footprint "R_1808"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 1808 (4520 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: datasheet page 3, https://product.tdk.com/system/files/dam/doc/product/capacitor/ceramic/mlcc/catalog/mlcc_commercial_soft_en.pdf), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -2.1 0)
		(layer "F.SilkS")
		(uuid "23cb933b-64e0-4ed8-831a-683ecf236445")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "C_1808"
		(at 0 2.1 0)
		(layer "F.Fab")
		(uuid "eeaf0e92-a597-47ab-9325-688c807df7d0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "6441ec78-1b4a-4a67-a343-05128df943cc")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "0040a5e3-a4d7-43a3-bd5b-0bfd93d9e0c2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -1.097369 -1.135)
		(end 1.097369 -1.135)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4b703a56-d616-421f-abb8-5feab962902d")
	)
	(fp_line
		(start -1.097369 1.135)
		(end 1.097369 1.135)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "aeb687b2-5884-426b-b05b-7d7c2b7adbc0")
	)
	(fp_rect
		(start -3.1 -1.4)
		(end 3.1 1.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "89fb2cfa-2069-44b5-9b93-f1c3ec213b74")
	)
	(fp_rect
		(start -2.275 -1.025)
		(end 2.275 1.025)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "425dde2c-8e2d-4230-987e-20508003a434")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "b65e2bcb-02cb-419c-a4ca-8fd9464fa31d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.075 0)
		(size 1.55 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16129)
		(uuid "add31033-87d9-4fcb-950f-54789ed90828")
	)
	(pad "2" smd roundrect
		(at 2.075 0)
		(size 1.55 2.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.16129)
		(uuid "0b7aa084-e1b4-4ed1-9ac7-4f91cc6191bf")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1808_4520Metric.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
