(footprint "CP_Elec_10x7.9"
	(version 20241229)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SMD capacitor, aluminum electrolytic, Panasonic F8, 10.0x7.9mm")
	(tags "capacitor electrolytic")
	(property "Reference" "REF**"
		(at 0 -6.2 0)
		(layer "F.SilkS")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "CP_Elec_10x7.9"
		(at 0 6.2 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -6.75 -2.46)
		(end -5.5 -2.46)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -6.125 -3.085)
		(end -6.125 -1.835)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.26 -4.195563)
		(end -5.26 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.26 -4.195563)
		(end -4.195563 -5.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.26 4.195563)
		(end -5.26 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -5.26 4.195563)
		(end -4.195563 5.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.195563 -5.26)
		(end 5.26 -5.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -4.195563 5.26)
		(end 5.26 5.26)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 5.26 -5.26)
		(end 5.26 -1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start 5.26 5.26)
		(end 5.26 1.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
	)
	(fp_line
		(start -6.8 -1.2)
		(end -6.8 1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -6.8 1.2)
		(end -5.4 1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.4 -4.25)
		(end -5.4 -1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.4 -4.25)
		(end -4.25 -5.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.4 -1.2)
		(end -6.8 -1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.4 1.2)
		(end -5.4 4.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.4 4.25)
		(end -4.25 5.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.25 -5.4)
		(end 5.4 -5.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -4.25 5.4)
		(end 5.4 5.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 5.4 -5.4)
		(end 5.4 -1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 5.4 -1.2)
		(end 6.8 -1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 5.4 1.2)
		(end 5.4 5.4)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 6.8 -1.2)
		(end 6.8 1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start 6.8 1.2)
		(end 5.4 1.2)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
	)
	(fp_line
		(start -5.15 -4.15)
		(end -5.15 4.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -5.15 -4.15)
		(end -4.15 -5.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -5.15 4.15)
		(end -4.15 5.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.558325 -1.7)
		(end -3.558325 -1.7)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.15 -5.15)
		(end 5.15 -5.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.15 5.15)
		(end 5.15 5.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start -4.058325 -2.2)
		(end -4.058325 -1.2)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_line
		(start 5.15 -5.15)
		(end 5.15 5.15)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
	)
	(fp_circle
		(center 0 0)
		(end 5 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at -4.35 0)
		(size 4.4 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.131579)
	)
	(pad "2" smd roundrect
		(at 4.35 0)
		(size 4.4 1.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.131579)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_10x7.9.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
