(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Opi_CM4"
		(pin_names
			(offset 6)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at 1.5 1.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" ""
			(at 0 -2.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 -2.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 0 -2.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 -2.5 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "ki_locked" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "Opi_CM4_1_0"
			(pin passive line
				(at -2.5 -10 0)
				(length 2.5)
				(name "PHY0_MDI_3+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -15 0)
				(length 2.5)
				(name "PHY0_MDI_3-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -20 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -25 0)
				(length 2.5)
				(name "PHY0_MDI_2-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "9"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -30 0)
				(length 2.5)
				(name "PHY0_MDI_2+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -35 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "13"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -40 0)
				(length 2.5)
				(name "PHY0_LED2/CFG_LDO1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "15"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -45 0)
				(length 2.5)
				(name "PHY0_LED1/CFG_LDO0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "17"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -50 0)
				(length 2.5)
				(name "PHY0_LED0/CFG_EXT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "19"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -55 0)
				(length 2.5)
				(name "DIY_LED"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -60 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "23"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -65 0)
				(length 2.5)
				(name "GPIO3_D1(I2S1_SDO_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "25"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -70 0)
				(length 2.5)
				(name "(I2S1_SDI_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "27"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -75 0)
				(length 2.5)
				(name "GPIO3_D5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "29"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -80 0)
				(length 2.5)
				(name "GPIO4_C0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "31"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -85 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "33"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -90 0)
				(length 2.5)
				(name "GPIO1_A1(I2C3_SCL_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "35"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -95 0)
				(length 2.5)
				(name "GPIO3_D6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "37"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -100 0)
				(length 2.5)
				(name "GPIO4_A6(SPI3_CS0_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "39"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -105 0)
				(length 2.5)
				(name "GPIO4_A4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "41"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -110 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "43"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -115 0)
				(length 2.5)
				(name "GPIO4_A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "45"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -120 0)
				(length 2.5)
				(name "GPIO4_A3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "47"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -125 0)
				(length 2.5)
				(name "GPIO3_C7(I2S1_SCLK_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "49"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_1_1"
			(rectangle
				(start 0 0)
				(end 50 -130)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -2.5 -5 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -5 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -10 180)
				(length 2.4892)
				(name "PHY0_MDI_1+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -15 180)
				(length 2.4892)
				(name "PHY0_MDI_1-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -20 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -25 180)
				(length 2.5)
				(name "PHY0_MDI_0-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "10"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -30 180)
				(length 2.5)
				(name "PHY0_MDI_0+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -35 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -40 180)
				(length 2.5)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "16"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -45 180)
				(length 2.5)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "18"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -50 180)
				(length 2.5)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "20"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -55 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -60 180)
				(length 2.5)
				(name "GPIO3_D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -65 180)
				(length 2.5)
				(name "GPIO3_D0(I2S1_LRCK_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "26"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -70 180)
				(length 2.5)
				(name "GPIO3_D7"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "28"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -75 180)
				(length 2.5)
				(name "GPIO3_D4"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "30"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -80 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "32"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -85 180)
				(length 2.4892)
				(name "GPIO4_A5"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "34"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -90 180)
				(length 2.4892)
				(name "GPIO1_A0(I2C3_SDA_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "36"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -95 180)
				(length 2.4892)
				(name "GPIO4_B3(SPI3_CLK_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "38"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -100 180)
				(length 2.4892)
				(name "GPIO4_B0(SPI3_MISO_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "40"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -105 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "42"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -110 180)
				(length 2.4892)
				(name "GPIO4_B2(SPI3_MOSI_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "44"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -115 180)
				(length 2.4892)
				(name "GPIO4_A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "46"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -120 180)
				(length 2.4892)
				(name "GPIO4_A0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "48"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -125 180)
				(length 2.4892)
				(name "GPIO3_C6(I2S1_MCLK_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "50"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_2_1"
			(rectangle
				(start 0 0)
				(end 50 -130)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -2.5 -5 0)
				(length 2.4892)
				(name "GPIO0_D0_(UART2_RX_M0)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "51"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -10 0)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "53"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -15 0)
				(length 2.4892)
				(name "GPIO0_D1_(UART2_TX_M0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "55"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -20 0)
				(length 2.4892)
				(name "SDMMC0_CLK"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "57"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -25 0)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "59"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -30 0)
				(length 2.4892)
				(name "SDMMC0_D3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "61"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -35 0)
				(length 2.4892)
				(name "SDMMC0_D0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "63"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -40 0)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "65"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -45 0)
				(length 2.4892)
				(name "SDMMC0_D1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "67"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -50 0)
				(length 2.4892)
				(name "SDMMC0_D2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "69"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -55 0)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "71"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -60 0)
				(length 2.4892)
				(name "SD_PWR_ON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "75"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -65 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "77"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -70 0)
				(length 2.4892)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "73"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -75 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "79"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -80 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "81"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -85 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "83"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -90 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "85"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_in line
				(at -2.5 -95 0)
				(length 2.4892)
				(name "VBUS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "87"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -100 0)
				(length 2.4892)
				(name "WL_nDIS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "89"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -105 0)
				(length 2.4892)
				(name "BT_nDIS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "91"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -110 0)
				(length 2.4892)
				(name "BOOT-SW"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "93"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -115 0)
				(length 2.4892)
				(name "WORK_LED"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "95"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -120 0)
				(length 2.4892)
				(name "CAMERA_PDN_L"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "97"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -125 0)
				(length 2.4892)
				(name "PMIC_PWRON"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "99"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -5 180)
				(length 2.4892)
				(name "nEXTRST"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "100"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -10 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "98"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -15 180)
				(length 2.4892)
				(name "SARADC_VIN2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "96"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -20 180)
				(length 2.4892)
				(name "SARADC_VIN3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "94"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -25 180)
				(length 2.4892)
				(name "RESETn"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "92"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 52.5 -30 180)
				(length 2.4892)
				(name "VCC_1V8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "90"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 52.5 -35 180)
				(length 2.4892)
				(name "VCC_1V8"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "88"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 52.5 -40 180)
				(length 2.4892)
				(name "VCC_3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "86"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin power_out line
				(at 52.5 -45 180)
				(length 2.4892)
				(name "VCC_3V3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "84"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -50 180)
				(length 2.4892)
				(name "I2C1_SDA_M0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "82"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -55 180)
				(length 2.4892)
				(name "I2C1_SCL_M0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "80"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -60 180)
				(length 2.4892)
				(name "VCCIO6"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "78"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -65 180)
				(length 2.4892)
				(name "SDMMC0_DET_L"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "76"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -70 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "74"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -75 180)
				(length 2.4892)
				(name "PWM7_IR"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "72"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -80 180)
				(length 2.4892)
				(name "SARADC_VIN1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "70"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -85 180)
				(length 2.4892)
				(name "SW_RECOVERY"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "68"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -90 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "66"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -95 180)
				(length 2.4892)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "64"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -100 180)
				(length 2.4892)
				(name "SDMMC0_CMD"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "62"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -105 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "60"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -110 180)
				(length 2.4892)
				(name "GPIO4_B4(I2C2_SDA_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "58"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -115 180)
				(length 2.4892)
				(name "GPIO4_B5(I2C2_SCL_M1)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "56"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -120 180)
				(length 2.4892)
				(name "GPIO4_C3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "54"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -125 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "52"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_3_0"
			(pin passive line
				(at -2.5 -10 0)
				(length 2.5)
				(name "USB_OTG0_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "103"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -15 0)
				(length 2.5)
				(name "USB_OTG0_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "105"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -20 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "107"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -25 0)
				(length 2.5)
				(name "PCIE20_PERSTn_3V3_L"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "109"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -30 0)
				(length 2.5)
				(name "Reserved"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "111"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -35 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "113"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -40 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D0N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "115"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -45 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "117"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -50 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "119"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -55 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "121"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -60 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "123"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -65 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "125"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -70 0)
				(length 2.5)
				(name "MIPI_CSI_RX_CLK0N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "127"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -75 0)
				(length 2.5)
				(name "MIPI_CSI_RX_CLK0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "129"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -80 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "131"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -85 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "133"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -90 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "135"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -95 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "137"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -100 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "139"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -105 0)
				(length 2.5)
				(name "MIPI_CSI_RX_D3P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "141"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -110 0)
				(length 2.5)
				(name "EDP_TX_D3P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "143"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -115 0)
				(length 2.5)
				(name "EDP_SDA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "145"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -120 0)
				(length 2.5)
				(name "EDP_SCL"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "147"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -125 0)
				(length 2.5)
				(name "EDP_TX_D3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "149"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_3_1"
			(rectangle
				(start 0 0)
				(end 50 -130)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -2.5 -5 0)
				(length 2.5)
				(name "USB_OTG0_ID"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "101"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -5 180)
				(length 2.4892)
				(name "PCIE20_CLKRE"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "102"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -10 180)
				(length 2.4892)
				(name "PCIE20_WAKEn"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "104"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -15 180)
				(length 2.4892)
				(name "GPIO4_A7/CA"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "106"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -20 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "108"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -25 180)
				(length 2.5)
				(name "PCIE20_REFCLKP_P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "110"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -30 180)
				(length 2.5)
				(name "PCIE20_REFCLKP_N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "112"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -35 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "114"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -40 180)
				(length 2.5)
				(name "PCIE20_RXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "116"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -45 180)
				(length 2.5)
				(name "PCIE20_RXN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "118"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -50 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "120"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -55 180)
				(length 2.5)
				(name "PCIE20_TXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "122"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -60 180)
				(length 2.5)
				(name "PCIE20_TXN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "124"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -65 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "126"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -70 180)
				(length 2.5)
				(name "MIPI_CSI_RX_D2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "128"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -75 180)
				(length 2.5)
				(name "MIPI_CSI_RX_D2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "130"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -80 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "132"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -85 180)
				(length 2.4892)
				(name "MIPI_CSI_RX_D3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "134"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -90 180)
				(length 2.4892)
				(name "MIPI_CSI_RX_D3P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "136"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -95 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "138"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -100 180)
				(length 2.4892)
				(name "MIPI_CSI_RX_CLK1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "140"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -105 180)
				(length 2.4892)
				(name "MIPI_CSI_RX_CLK1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "142"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -110 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "144"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -115 180)
				(length 2.4892)
				(name "EDP_TX_D2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "146"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -120 180)
				(length 2.4892)
				(name "EDP_TX_D2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "148"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -125 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "150"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_4_0"
			(pin passive line
				(at -2.5 -10 0)
				(length 2.5)
				(name "RT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "153"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -15 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "155"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -20 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_D0N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "157"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -25 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_D0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "159"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -30 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "161"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -35 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_D1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "163"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -40 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_D1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "165"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -45 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "167"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -50 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_CLKN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "169"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -55 0)
				(length 2.5)
				(name "MIPI_DSI_TX0_CLKP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "171"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -60 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "173"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -65 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D0N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "175"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -70 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "177"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -75 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "179"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -80 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "181"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -85 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "183"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -90 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "185"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -95 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_CLKN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "187"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -100 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_CLKP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "189"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -105 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "191"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -110 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D2N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "193"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -115 0)
				(length 2.5)
				(name "MIPI_DSI_TX1_D2P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "195"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -120 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "197"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -125 0)
				(length 2.5)
				(name "HDMI_TXDDC_SDA_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "199"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_4_1"
			(rectangle
				(start 0 0)
				(end 50 -130)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -2.5 -5 0)
				(length 2.5)
				(name "HDMI_CEC_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "151"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -5 180)
				(length 2.4892)
				(name "EDP_TX_D1P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "152"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -10 180)
				(length 2.4892)
				(name "EDP_TX_D1N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "154"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -15 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "156"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -20 180)
				(length 2.4892)
				(name "EDP_TX_D0P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "158"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -25 180)
				(length 2.5)
				(name "EDP_TX_D0N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "160"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -30 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "162"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -35 180)
				(length 2.5)
				(name "EDP_TX_AUXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "164"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -40 180)
				(length 2.5)
				(name "EDP_TX_AUXN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "166"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -45 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "168"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -50 180)
				(length 2.5)
				(name "HDMI_TX2P_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "170"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -55 180)
				(length 2.5)
				(name "HDMI_TX2N_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "172"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -60 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "174"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -65 180)
				(length 2.5)
				(name "HDMI_TX1P_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "176"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -70 180)
				(length 2.5)
				(name "HDMI_TX1N_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "178"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -75 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "180"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -80 180)
				(length 2.4892)
				(name "HDMI_TX0P_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "182"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -85 180)
				(length 2.4892)
				(name "HDMI_TX0N_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "184"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -90 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "186"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -95 180)
				(length 2.4892)
				(name "HDMI_TXCLKP_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "188"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -100 180)
				(length 2.4892)
				(name "HDMI_TXCLKN_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "190"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -105 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "192"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -110 180)
				(length 2.4892)
				(name "MIPI_DSI_TX1_D3N"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "194"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -115 180)
				(length 2.4892)
				(name "MIPI_DSI_TX1_D3P"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "196"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -120 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "198"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -125 180)
				(length 2.4892)
				(name "HDMI_TXDDC_SCL_PORT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "200"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_5_0"
			(pin passive line
				(at -2.5 -10 0)
				(length 2.5)
				(name "USB2_HOST3_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "203"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -15 0)
				(length 2.5)
				(name "USB2_HOST3_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "205"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -20 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "207"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -25 0)
				(length 2.5)
				(name "USB2_HOST2_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "209"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -30 0)
				(length 2.5)
				(name "USB2_HOST2_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "211"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -35 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "213"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -40 0)
				(length 2.5)
				(name "HP_DET_L"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "215"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -45 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "217"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -50 0)
				(length 2.5)
				(name "USB3_HOST1_DM"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "219"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -55 0)
				(length 2.5)
				(name "USB3_HOST1_DP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "221"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at -2.5 -60 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "223"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(symbol "Opi_CM4_5_1"
			(rectangle
				(start 0 0)
				(end 50 -65)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(pin passive line
				(at -2.5 -5 0)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "201"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -5 180)
				(length 2.4892)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "202"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -10 180)
				(length 2.4892)
				(name "HPR_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "204"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -15 180)
				(length 2.4892)
				(name "HPL_OUT"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "206"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -20 180)
				(length 2.4892)
				(name "HP_SNS"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "208"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -25 180)
				(length 2.5)
				(name "MIC1_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "210"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -30 180)
				(length 2.5)
				(name "MIC2_IN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "212"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -35 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "214"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -40 180)
				(length 2.5)
				(name "USB3_HOST1_SSTXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "216"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -45 180)
				(length 2.5)
				(name "USB3_HOST1_SSTXN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "218"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -50 180)
				(length 2.5)
				(name "GND"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "220"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -55 180)
				(length 2.5)
				(name "USB3_HOST1_SSRXP"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "220"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin passive line
				(at 52.5 -60 180)
				(length 2.5)
				(name "USB3_HOST1_SSRXN"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "224"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
