(footprint "VSSOP-8_2.3x2mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "VSSOP, 8 Pin (https://www.jedec.org/standards-documents/docs/mo-187-f), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "VSSOP SO JEDEC-MO-187-CA Texas_DCU0008A")
	(property "Reference" "REF**"
		(at 0.4318 -2.1844 0)
		(layer "F.SilkS")
		(uuid "1c64bb0e-f130-4a1b-86a8-be3c0f424ccb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "VSSOP-8_2.3x2mm_P0.5mm"
		(at 0 1.95 0)
		(layer "F.Fab")
		(uuid "e42bf72c-8e13-4c10-8631-4078e3a24245")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "684c716d-3dde-4664-ae8f-8d5c0e0631e9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d1768cd9-d71d-4ecc-8be6-ff3474449e31")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.7112 -1.185)
		(end -0.7874 -1.0922)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a3c96b0b-dde4-4277-95d7-d392188f5215")
	)
	(fp_line
		(start -0.6858 -1.185)
		(end 1.26 -1.185)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bf30719a-e2ac-4cc5-9438-8756953652ae")
	)
	(fp_line
		(start 1.26 1.185)
		(end -1.26 1.185)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "78f16aba-1a82-4547-8dda-6bd9ebcdc16c")
	)
	(fp_circle
		(center -1.397 -1.3462)
		(end -1.297 -1.3462)
		(stroke
			(width 0.2)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "caa3f840-c20d-4394-a71a-197572eb975d")
	)
	(fp_line
		(start -2.28 -1.18)
		(end -1.4 -1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c29d5608-9aff-4a7f-b1a2-812bed30a630")
	)
	(fp_line
		(start -2.28 1.18)
		(end -2.28 -1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99e4a255-5a14-4314-b817-0034a3f6190b")
	)
	(fp_line
		(start -1.4 -1.25)
		(end 1.4 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a1b1d2a8-f1ee-4388-8c7e-cf9b7fbf0a3c")
	)
	(fp_line
		(start -1.4 -1.18)
		(end -1.4 -1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ce9429c5-55a0-4931-aee4-1dbf47f54679")
	)
	(fp_line
		(start -1.4 1.18)
		(end -2.28 1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "3d9d892f-8265-435d-a81e-994d32ac6738")
	)
	(fp_line
		(start -1.4 1.25)
		(end -1.4 1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "be688c5f-cf5f-43f9-a4a0-a7cffea458d5")
	)
	(fp_line
		(start 1.4 -1.25)
		(end 1.4 -1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6baee126-a25f-4c8f-911c-51cc1ea6720e")
	)
	(fp_line
		(start 1.4 -1.18)
		(end 2.28 -1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "120d24cb-e8bb-4191-9114-3566c634790a")
	)
	(fp_line
		(start 1.4 1.18)
		(end 1.4 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ddf2f034-93f8-49a1-8ce5-41dfc876fd97")
	)
	(fp_line
		(start 1.4 1.25)
		(end -1.4 1.25)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "83b545dc-8bea-4444-8235-e020da0673a7")
	)
	(fp_line
		(start 2.28 -1.18)
		(end 2.28 1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c618d234-532d-4881-9f1f-8810d68ff008")
	)
	(fp_line
		(start 2.28 1.18)
		(end 1.4 1.18)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b660abaa-73c3-4a77-9ecd-e808a8066a45")
	)
	(fp_poly
		(pts
			(xy -0.65 -1) (xy 1.15 -1) (xy 1.15 1) (xy -1.15 1) (xy -1.15 -0.5)
		)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "9e2fa451-5fac-46df-978b-303032f874a3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "5c590d02-3385-4272-a11a-826af4f40967")
		(effects
			(font
				(size 0.57 0.57)
				(thickness 0.09)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.4 -0.75)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ca04f62a-5281-46ff-8f16-6f6fdd527c6a")
	)
	(pad "2" smd roundrect
		(at -1.4 -0.25)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "c25a8da9-ac58-4db3-b12c-9983300fb75e")
	)
	(pad "3" smd roundrect
		(at -1.4 0.25)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "b2d31fae-d89e-4a44-b138-1785f8bff8d8")
	)
	(pad "4" smd roundrect
		(at -1.4 0.75)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "cb7b3cf2-6588-4165-8d2a-092c8164b0aa")
	)
	(pad "5" smd roundrect
		(at 1.4 0.75)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "7ae4aed1-53c2-4344-99b8-932e4c046f98")
	)
	(pad "6" smd roundrect
		(at 1.4 0.25)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5dac496f-f1ca-4c2c-9e51-c43b829ea878")
	)
	(pad "7" smd roundrect
		(at 1.4 -0.25)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "66c947b8-022d-4280-a32e-dc7b2b5826f3")
	)
	(pad "8" smd roundrect
		(at 1.4 -0.75)
		(size 1.25 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "2137cc47-72f0-4c75-9bdd-4ea182ca54ae")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/VSSOP-8_2.3x2mm_P0.5mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
