(footprint "Opi_cm4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Raspberry Pi 4 Compute Module")
	(tags "Raspberry Pi 4 Compute Module")
	(property "Reference" "REF**"
		(at 37.8 -4.1 270)
		(layer "F.SilkS")
		(uuid "6ba95e0a-c495-4977-a467-dc05254d4a6c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "Opi_cm4"
		(at 16.52 0.19 0)
		(layer "F.Fab")
		(uuid "ecf46533-bd5b-4090-97e5-8a00f065ac4d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "7d8229a2-bcb3-4c70-8e06-2a7729e7776e")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "a14135d2-84ec-46b6-b69f-5363b154a336")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -3.5 -48)
		(end -3.5 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "03a45250-7a4b-479b-8483-3036933abe03")
	)
	(fp_line
		(start 0 3.5)
		(end 33 3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "4880913a-5777-4185-a561-22b3627ae519")
	)
	(fp_line
		(start 33 -51.5)
		(end 0 -51.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e4888339-9e62-4047-8200-f947957418e6")
	)
	(fp_line
		(start 36.5 0)
		(end 36.5 -48)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "98f5b519-b57f-443c-8809-c93df1cb89b5")
	)
	(fp_arc
		(start -3.5 -48)
		(mid -2.474874 -50.474874)
		(end 0 -51.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cdecba76-9ea7-4eb1-ab88-26beaa2b8756")
	)
	(fp_arc
		(start 0 3.5)
		(mid -2.474874 2.474874)
		(end -3.5 0)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "fedebfdd-8d1f-4a81-8c86-479e797f6f08")
	)
	(fp_arc
		(start 33 -51.5)
		(mid 35.474874 -50.474874)
		(end 36.5 -48)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b492fd46-b146-491c-ad21-a185f9fc29bd")
	)
	(fp_arc
		(start 36.5 0)
		(mid 35.474874 2.474874)
		(end 33 3.5)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a12bba9c-ebcf-4c75-b10f-938883aae532")
	)
	(fp_line
		(start -1.8484 -31.7337)
		(end 0 0)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "e986b7f3-c173-4660-be0c-38fb09e6ea68")
	)
	(fp_line
		(start 0 0)
		(end 13.8593 -49.927)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "b386eea1-d97f-4bfd-a53f-607a881629e7")
	)
	(fp_line
		(start 0 0)
		(end 32.1506 -31.7348)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "Dwgs.User")
		(uuid "fd1b2d1a-d117-484c-8418-735470314c20")
	)
	(fp_line
		(start -3.5 -51.5)
		(end 36.5 -51.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "9f54fe93-81a0-46a7-b31e-5b4727fd261c")
	)
	(fp_line
		(start -3.5 3.5)
		(end -3.5 -51.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5a4b5d56-aef1-408f-bb01-536d13e2267a")
	)
	(fp_line
		(start 36.5 -51.5)
		(end 36.5 3.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "dec3b26a-1b47-48f2-b6ca-cac60ef89d0c")
	)
	(fp_line
		(start 36.5 3.5)
		(end -3.5 3.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "8fb3a07b-9b53-464f-a223-06f665eb4b25")
	)
	(fp_text user "2"
		(at 19.5 -46.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "0441e0e9-67c9-4b8c-85f0-ad13334548dc")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "JP1"
		(at 2.5 -20.4 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "29cf88ff-f901-466b-bc92-ff68983f23e8")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "100"
		(at 2.5 -10.4 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "34a954c5-0c01-4ac2-906c-6338eb0cc1a2")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "1"
		(at 30.5 -30.7 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "3c934b88-fba4-41d7-ac2b-2e68e5e16247")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "JP3"
		(at 15.97 -46.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "44893623-cf29-44d4-97b5-b21f98f20859")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "99"
		(at 30.5 -11.1 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4defe40b-c216-4975-9fab-0df357aebad9")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "24"
		(at 13.5 -46.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "4f83a666-f07c-4001-a72c-ffc582c5bc91")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "JP2"
		(at 30.47 -20.4 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "a1b89cb9-9a37-4d1a-8fce-6e11fad406f0")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(fp_text user "2"
		(at 2.5 -30.8 90)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "b2f86742-9491-4e73-a20c-6019eba6398a")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
			(justify left)
		)
	)
	(pad "" np_thru_hole circle
		(at 0 -48)
		(size 2.7 2.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 1.7)
		(clearance 1.7)
		(uuid "c2c1d247-2c20-4b1e-a5d1-8d71cf195ab3")
	)
	(pad "" np_thru_hole circle
		(at 0 0)
		(size 2.7 2.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 1.7)
		(clearance 1.7)
		(uuid "0e9ff0ab-be9a-410e-83d3-560aabe41a96")
	)
	(pad "" np_thru_hole circle
		(at 33 -48)
		(size 2.7 2.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 1.7)
		(clearance 1.7)
		(uuid "24644d5b-8a8d-4e6c-81de-1d29e1b2cf87")
	)
	(pad "" np_thru_hole circle
		(at 33 0)
		(size 2.7 2.7)
		(drill 2.7)
		(layers "*.Cu" "*.Mask")
		(solder_mask_margin 1.7)
		(clearance 1.7)
		(uuid "bbef7c9c-3baf-44f1-a3db-387df8539077")
	)
	(embedded_fonts no)
	(model "${KI_3D}/Module/PCB-CM4.stp"
		(offset
			(xyz 16.5 24 3.15)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 90)
		)
	)
	(model "./CM4IO.3dshapes/DF40C-100DS.stp"
		(offset
			(xyz 33.46 15.38 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
