(footprint "USON-10_2.5x1.0mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USON-10 2.5x1.0mm_ Pitch 0.5mm http://www.ti.com/lit/ds/symlink/tpd4e02b04.pdf")
	(tags "USON-10 2.5x1.0mm Pitch 0.5mm")
	(property "Reference" "REF**"
		(at 0.01829 -2.5 0)
		(layer "F.SilkS")
		(uuid "fd779aab-8aca-4cfa-ba39-08cfb20ae844")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "USON-10_2.5x1.0mm_P0.5mm"
		(at 0.01829 2.5 0)
		(layer "F.Fab")
		(uuid "9dd20a68-917d-4e1d-9a56-c0745ce2bb9f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a481a5bf-0e49-4a0a-af6a-a50ca1f8f8b1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "25e06dd4-0e95-4792-be4a-bc0ac9b5d3da")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -0.29 -1.41)
		(end -0.4 -1.3)
		(stroke
			(width 0.15)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4a30e6a6-b993-4dcc-9f96-64f5a6d25295")
	)
	(fp_line
		(start 0.5 -1.41)
		(end -0.29 -1.41)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "a97577fc-5d82-48b5-9412-975135f4271f")
	)
	(fp_line
		(start 0.5 1.41)
		(end -0.5 1.41)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "0f508c13-fad2-4f35-912b-24be8c48a2da")
	)
	(fp_poly
		(pts
			(xy -0.85 -1.57) (xy -1.13 -1.57) (xy -0.85 -1.85) (xy -0.85 -1.57)
		)
		(stroke
			(width 0.12)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "31566dcc-530d-4fff-9001-289247f7bb8d")
	)
	(fp_line
		(start -0.91 -1.5)
		(end 0.91 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e1badb2e-9e88-4837-91b3-467f6d470bf2")
	)
	(fp_line
		(start -0.91 1.5)
		(end -0.91 -1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "82f3a98f-3bb8-40cf-806b-d034a8be0d94")
	)
	(fp_line
		(start 0.91 -1.5)
		(end 0.91 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "b6fb4868-06ee-4fb2-bfbe-0c55d35501d6")
	)
	(fp_line
		(start 0.91 1.5)
		(end -0.91 1.5)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "1657ef41-e24c-4a5b-be89-f8ee128f6a9c")
	)
	(fp_line
		(start -0.5 -1)
		(end -0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a9d1c62b-3a2d-4039-9a34-7dcaee3b8609")
	)
	(fp_line
		(start -0.5 1.25)
		(end 0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "5cb4eb0b-0580-438b-a2f0-80bc8bc6600a")
	)
	(fp_line
		(start -0.25 -1.25)
		(end -0.5 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4e856475-c8b7-430f-8cee-b1ec23578f3d")
	)
	(fp_line
		(start 0.5 -1.25)
		(end -0.25 -1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e65886c2-a3c2-4067-a316-2eaf40697253")
	)
	(fp_line
		(start 0.5 -1.25)
		(end 0.5 1.25)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "345527d7-bf9f-404a-97c5-cdab1ea7fce3")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
		(uuid "8747b04f-3f70-4b72-96b0-9ab37da02dc1")
		(effects
			(font
				(size 0.55 0.55)
				(thickness 0.1)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.385 -1 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "bb57532e-6dcd-4c07-a63c-7db00217baab")
	)
	(pad "2" smd roundrect
		(at -0.385 -0.5 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "1b25f17a-0f9f-4253-8858-bf501e2620d2")
	)
	(pad "3" smd roundrect
		(at -0.385 0 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "491feaff-f99f-4c97-8031-a8fb65f06c6e")
	)
	(pad "4" smd roundrect
		(at -0.385 0.5 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "2cd0f2fb-eba3-4cc9-9762-9653785aa775")
	)
	(pad "5" smd roundrect
		(at -0.385 1 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f6c6c7e2-5465-4eeb-b41b-cc808fbe4cbd")
	)
	(pad "6" smd roundrect
		(at 0.385 1 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "e8e5127f-8ba6-4868-9003-c4f96f04c66a")
	)
	(pad "7" smd roundrect
		(at 0.385 0.5 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "ad90af0c-598a-4a12-8ca4-468761371581")
	)
	(pad "8" smd roundrect
		(at 0.385 0 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "f9e0e3fe-00d9-44a5-bc57-845682132e8d")
	)
	(pad "9" smd roundrect
		(at 0.385 -0.5 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "9aeebf29-17d3-4deb-9fa9-0920da5c2c25")
	)
	(pad "10" smd roundrect
		(at 0.385 -1 270)
		(size 0.3 0.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5c26946b-97a0-4fc9-9e28-6b817dfd0888")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/USON-10_2.5x1.0mm_P0.5mm.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
